• Output Power Watt RMS
• 1 - Ohm 1200Wrms X 1
• 2 - Ohms 750 Wrms X 1
• 4 - Ohms 350 Wrms X 1
• Frequency Response 15Hz - 150Hz
• Signal to Noise Ratio 95dB
• THD % 0.10%
• Variable Low - Pass 40Hz - 150Hz
• Variable Subsonic Filter 15Hz - 55Hz
• 45Hz Bass Boost 0 -+ 12dB
• Input ( RCA Jack )
• Bass Boost Remote Control